Teahaus Assembly

Extra notes:

Where to use the different rubber seals:

- Rubber V112 - see appendix mail

- Rubber V23 - Page 64, 65 and 98

- Rubber V114 - all KPT-grills and TR-grills on the inside (for example Page 58 und 59) they called on this page "system gasket"

- Rubber V98 - all "covering profile 6 mm" (P12, P16, P17, P18, P)

- Rubber V41 - around doorframe and window frame

- Rubber V42 - all edge grills and TR-grills on the outside